**Underground Vibration Classification: PCB**

1. **FUNCTION:** For our project, we decided to incorporate the necessary DC offset circuit as our PCB requirement. To obtain vibration oscillations, the geophone sensors need to be offset to capture both the peaks and troughs of the vibrations. Without this offset, the Arduino’s analog-to-digital converter only capture the peaks of the vibrations, while the troughs are not captured and recorded as zero-point values. The functionality of the PCB will be to offset the geophone data by half the operational voltage of the Arduino microcontroller. The capacitors in our schematic serve to block any DC voltages from the Arduino from getting into the geophone sensors and the identical resistor values form a voltage divider that offsets the vibrations by half of the operational voltage of the Arduino.
2. **Schematic Diagram:**

Diagram, schematic

Description automatically generated

A picture containing text, electronics, circuit

Description automatically generated

Figure 2 - PCB schematic made in Altium.

Figure – Circuit schematic made in Altium.

1. **Production File and Ordering Information**

**Timeline

Description automatically generated**

* Company is called JLCPCB.
* Cost was only $2.00 for 5pcs.
* Shipping costs $17.80
* Build Time is going to be able 3 days.
* Shipping will take about 4-7 business days.

1. **PCB Integration:**

Our team plans to implement our PCB design within the next coming weeks. As soon as we receive the PCBs either Gus or Tyler will be able to solder them into our system design. We plan to validate and test the PCBs as soon we can get our hands on them.